EVER-FABRIC™ is a 100% polyester reinforcement, stitch bond 2.98 oz. fabric used in all deck coating systems, emulsion asphalt roof coatings, acrylic, silicone, urethane and all other elastomeric, liquid-applied roof coatings. EVERFABRIC™ adds tremendous strength and reinforcement to any elastomeric liquid-applied roof coating system including the Ever-Thane Cool Roof System, the Sil-Thane Cool Roof System, the Ever-Silic Cool Roof System and the Ever-Crylic Cool Roof System.

FEATURES & BENEFITS

EVER-FABRIC™ is designed to reinforce cracks, seams, joints, large openings, gaps, splits, and tears in any deck and roof system. Helps build strength in drains, scuppers, penetrations, transitions and flashing detail in all types of roof restoration systems.

FABRIC SIZES

STORAGE & HANDLING

Store EVER-FABRIC™ in a dry, cool place away from direct sunlight, heat, sparks, open flame,

and moisture. Keep off concrete floor.

SAFETY

Use appropriate protective clothing, hand and eye protection. This product is intended for industrial use by properly trained professional applicators only. Do not use in food grade systems or potable water. Please read all information in the general guidelines, technical data sheets, application guide, and material safety data sheets (MSDS) before applying EVER FABRIC™ in any of EVER-THANE® Systems, EVER-SILIC® Systems, EVER-CRYLIC® Systems and/ or any other elastomeric roof and decking system. Published technical data and instructions are subject to change without notice. Contact your local EVERROOF® representative or visit our website for current technical data and instructions.