ADHESIVE/PRIMER

DESCRIPTION

ADHESIVE/PRIMER is a waterborne modified acrylic primer specifically designed to provide maximum adhesion of polyester reinforcing fabric and coatings to various construction surfaces. ADHESIVE PRIMER is resistant to asphaltic bleed through and may be applied to BUR roofing, concrete, plywood and some metallic surfaces. Substrates to receive primer should be clean, dry and free of any foreign material such as grease, oil, water, dirt, etc. ADHESIVE PRIMER is fast-drying and has little or no smell associated with its application.

APPLICATION

ADHESIVE PRIMER application rates will vary depending on substrates. ADHESIVE PRIEMER can be applied with airless spray equipment, brush, or roller. The primer must be thoroughly mixed prior to application. Cleanup can be accomplished with either water or mineral spirits.

FEATURES

Odorless

Nonflammable

Nonhazardous

Minimum overspray

Optimum adhesion characteristics

(if used as directed)

TYPICAL USES

ADHESIVE PRIMER is compatible with Everroof’s foam and most coatings. For information regarding coatings that are not specified in this data sheet, please contact EVERROOF™.

DIRECTION FOR USE

MIXING: ADHESIVE PRIMER should be thoroughly mixed just before application and applied to a clean, dry surface.

ADHESIVE PRIMER is designed for airless spray equipment, brush or roller.

Minimum Temperature: 38°F.

Thinning: None normally required.

Clean-up Solvent: Water or mineral spirits.