EVERROOF™ PRIMER SP10 is a waterborne modified acrylic neoprene asphalt primer specifically designed to provide maximum adhesion of polyurethane foam and coatings to various construction surfaces. When directly applied to polyurethane foam it provides short-term protection from the elements and an excellent surface for bonding of additional urethane foam or coatings.

FEATURES & BENEFITS

EVERROOF™ PRIMER SP10 may be applied to BUR roofing, concrete, plywood and some metallic surfaces. Substrates to receive primer must be clean, dry and free of any foreign material such as grease, oil, water, dirt, etc. It is fast-drying and has little or no smell associated with its application.

Odorless

Nonflammable

Nonhazardous

Minimum Overspray

Optimum Adhesion Characteristics

DIRECTION OF USE

APPLICATION: EVERROOF™ PRIMER SP10 should be applied at a rate of 1/4 gallon per 100 square feet. NOTE: Application rates will vary depending on substrates. It can be applied with airless spray equipment such as Graco 30:1. The primer must be thoroughly mixed prior to application. Cleanup can be accomplished with either water or mineral spirits.

COMPATABILITY: EVERROOF™ PRIMER SP10 is compatible with EverRoof™ foam and most coatings. For information regarding coatings that are not specified in this data sheet, please contact EverRoof™.

PACKAGING / SHIPPING:

5 gallon pails and 55 gallon drums

Approximate Shipping Weight – 10 lbs. / gallon

Freight Classification – paint, non-hazardous